Caption: 
SwRI used internal funding to develop SwSCOR’s three-stage lens system mounted behind a single-pylon external occulter to minimize distortion across the field of view. A polarizer wheel is placed in front of the first lens. The current Phase A study will study options for the external occulter.