Caption: 
SwRI-developed remote neutrally buoyant sensors float through an underground cave or conduit and measure the path, dimensions and morphology of the void using an array of ultrasound sensors.