Caption: 
The SwRI-designed internally cooled compressor diaphragm has been shown to reduce compression power requirements by as much as 25 percent.

Credit: 
Image Courtesy of Southwest Research Institute