Caption: 
A methane plume (red and blue) was captured with a midwave infrared imager. SwRI will quantify fugitive methane flow rates using machine learning, thermal imaging and lidar technology.

Credit: 
Courtesy of Southwest Research Institute