Caption: 
The Stoichiometric ECTO-Lab heat exchanger assembly undergoes final torque checks in SwRI’s Exhaust Composition Transient Operation Laboratory, a state-of-the-art, computer-controlled, multi-fueled burner system to simulate engine exhaust conditions.

Credit: 
Courtesy of Southwest Research Institute 