Caption: 
A technician connects a sample line to monitor ECTO-Lab back pressure. SwRI’s Exhaust Composition Transient Operation Laboratory is a state-of-the-art, computer-controlled, multi-fueled burner system to simulate engine exhaust conditions.

Credit: 
Courtesy of Southwest Research Institute