Caption: 
An SwRI engineer adjusts the ignition system used for initially heating the recently commissioned circulating fluidized bed pilot plant to 650°C for high temperature thermal fast pyrolysis. SwRI’s CFB system is equipped to handle fast pyrolysis for biomas