Caption: 
The Heavy Article Test now has 14,350 square feet of working space. The facility expansion included adding a fully controllable air exhaust system for removing heat and fumes, and a 95-ton capacity air-cooled water chiller.

Credit: 
Image Courtesy of Southwest Research Institute