Caption: 
The newly completed Flow Component Test Cell, which measures 15-feet wide by 15-feet deep and 25-feet high, has a five-ton crane and a large equipment door to accommodate heavy test articles.

Credit: 
Courtesy of Southwest Research