Caption: 
The SwRI-developed superhydrophobic coatings are produced using a vacuum process that allows them to form a thin, glass-like durable coating on pipe surfaces. 

Credit: 
Image Courtesy of Southwest Research Institute