Caption: 
SwRI developed and delivered the LMS instrument for the Mare Crisium lander to determine the electrical conductivity of the interior of the Moon by measuring low-frequency electric and magnetic fields. LMS includes (from left) a magnetometer (white) on an extendable mast, a central electronics box and four spring-launched electrodes.