Caption: 
The user-friendly MsT sensor automatically adjusts frequencies to inspect structures, which reduces human error. At just 1.1 inches wide, MsT can squeeze into compact areas. The MsT can now scan a structure in segments, providing more precise and thorough inspections.  

Credit: 
Image Courtesy of Southwest Research Institute